# simulcast
demonstrates of how to handle incoming track with multiple simulcast rtp streams and show all them back.

The browser will not send higher quality streams unless it has the available bandwidth. You can look at
the bandwidth estimation in `chrome://webrtc-internals`. It is under `VideoBwe` when `Read Stats From: Legacy non-Standard`
is selected.

## Instructions
### Download simulcast
```
go install github.com/pion/webrtc/v4/examples/simulcast@latest
```

### Open simulcast example page
[jsfiddle.net](https://jsfiddle.net/tz4d5bhj/) you should see two text-areas and two buttons: `Copy browser SDP to clipboard`, `Start Session`.

### Run simulcast, with your browsers SessionDescription as stdin
In the jsfiddle the top textarea is your browser's Session Description. Press `Copy browser SDP to clipboard` or copy the base64 string manually.
We will use this value in the next step.

#### Linux/macOS
Run `echo $BROWSER_SDP | simulcast`
#### Windows
1. Paste the SessionDescription into a file.
1. Run `simulcast < my_file`

### Input simulcast's SessionDescription into your browser
Copy the text that `simulcast` just emitted and copy into second text area

### Hit 'Start Session' in jsfiddle, enjoy your video!
Your browser should send a simulcast track to Pion, and then all 3 incoming streams will be relayed back.

Congrats, you have used Pion WebRTC! Now start building something cool
